PRODUCTION PERFORMANCE MONITORING WORKFLOW FOR MANUFACTURERS

Created by ChecklistGuro (https://checklistguro.com)

[ ] Retrieve Production Data: Fetch production data from the MES system for the previous shift.
[ ] Calculate OEE: Aggregate data to calculate Overall Equipment Effectiveness (OEE).
[ ] Calculate Yield Rate: Aggregate data to calculate the yield rate for the production run.
[ ] Get Planned Production Schedule: Retrieve the planned production schedule for comparison.
[ ] Calculate Variance from Plan: Calculate the difference between actual and planned production quantities.
[ ] Calculate Downtime Duration: Calculate total downtime duration based on recorded downtime events.
[ ] Log Performance Metrics: Create an entry in the performance metrics data model with calculated metrics.
[ ] Assign Review Task: Create a task for the production supervisor to review performance metrics.
[ ] Notify Supervisor of Key Deviations: Send an email to the production supervisor if OEE falls below a threshold.
[ ] Retrieve Previous Shift Performance: Get the performance data from the previous shift to enable comparison.
[ ] Generate Performance Report: Create a report summarizing the current shift's performance.
[ ] Assign Root Cause Analysis Task (if needed): Create a task for engineering if performance falls outside acceptable parameters.
[ ] Update Shift Status: Update the status of the current shift in the system.

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/workflow-templates/manufacturing/production-performance-monitoring-workflow-for-manufacturers
(Click "Install Template" to launch your digital inspection tool immediately)