PUBLIC TRANSPORT DEPOT WORKSHOP TOOLING & EQUIPMENT CALIBRATION CHECKLIST 2026
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--- PRE-INSPECTION ADMINISTRATIVE VERIFICATION ---
[ ] Inspection Date
[ ] Inspector Name
[ ] Workshop Station/Zone (Heavy Engine Bay, Pneumatic Tool Station, Precision Measurement Lab, General Maintenance Area)
[ ] Master Equipment Inventory List
[ ] Pre-Inspection Documents Verified (Calibration Certificates, Technician Training Logs, Previous Inspection Reports, Tool Purchase Invoices)
[ ] Supervisor Authorization

--- PRECISION MEASURING INSTRUMENTS AUDIT ---
[ ] Last Calibration Date
[ ] Instrument Condition Status (Excellent, Good - Functional, Fair - Requires Maintenance, Poor - Out of Calibration)
[ ] Measured Deviation (mm/unit)
[ ] Detected Defects (Visible Wear, Corrosion/Rust, Missing Calibration Sticker, Physical Damage)
[ ] Detailed Inspection Findings
[ ] Technician Verification Signature

--- PNEUMATIC & HYDRAULIC EQUIPMENT INSPECTION ---
[ ] Inspection Date
[ ] Equipment ID/Serial Number
[ ] Equipment Type (Air Compressor, Hydraulic Press, Pneumatic Impact Wrench, Hydraulic Jack, Air Hose Reel)
[ ] Pressure Gauge Calibration Status (Pass - Within Calibration Date, Fail - Calibration Expired, Fail - Physical Damage Detected)
[ ] Visual Inspection Checklist (No visible leaks in hoses/seals, No signs of corrosion or rust, Pressure levels are within operating range, Safety valves are functional)
[ ] Defects or Discrepancies Found
[ ] Photo of Equipment Condition/Leakage
[ ] Technician Verification

--- POWER TOOL & ELECTRICAL SAFETY ASSESSMENT ---
[ ] Inspection Date
[ ] Tool ID/Asset Number (PTD-ELEC-001, PTD-ELEC-002, PTD-ELEC-003)
[ ] Safety Checkpoints Completed (Power Cord Integrity Check, Plug & Socket Condition, Switch & Trigger Functionality, Casing & Housing Damage Check, Earthing/Grounding Verification)
[ ] Voltage Reading Observed
[ ] Defects or Damage Observations
[ ] Photo of Tool Condition
[ ] Inspector Digital Signature

--- HEAVY LIFTING & HOISTING GEAR COMPLIANCE ---
[ ] Last Inspection Date
[ ] Hoist/Crane ID Number (Crane-01, Crane-02, Hoist-A, Hoist-B)
[ ] Safety Components Inspected (Wire Rope/Chain Integrity, Hook & Latch Functionality, Load Limit Switch Operation, Braking System Efficiency, Hydraulic Cylinder Seals)
[ ] Maximum Rated Load (kg)
[ ] Observed Wear or Damage Notes
[ ] Lead Technician Verification

--- DIAGNOSTIC & ELECTRONIC TESTING EQUIPMENT CHECK ---
[ ] Last Calibration Date
[ ] Diagnostic Tool Operational Status (Fully Operational, Requires Maintenance, Out of Calibration, Decommissioned)
[ ] Tested Components (OBD-II Scanners, Multimeters, Oscilloscopes, Battery Analyzers, Circuit Testers)
[ ] Error Margin/Deviation Detected (%)
[ ] Discrepancy Notes & Error Details
[ ] Upload Calibration Certificate/Report
[ ] Technician Verification Signature

--- WORKSHOP HAND TOOL MAINTENANCE & CONDITION ---
[ ] Tool Condition Status (Excellent (Ready for Use), Good (Minor Wear), Fair (Requires Cleaning/Maintenance), Poor (Damaged/Out of Service))
[ ] Identified Tool Defects
[ ] Last Cleaning/Service Date
[ ] Quantity of Tools Inspected
[ ] Damage Evidence Photo
[ ] Inspector Verification

--- CALIBRATION ENVIRONMENT & STORAGE STANDARDS ---
[ ] Storage Area ID/Zone (Zone A - Precision Instruments, Zone B - Heavy Machinery, Zone C - Hand Tools, Zone D - Hazardous Materials)
[ ] Measured Ambient Temperature (°C)
[ ] Humidity Level Status (Optimal, High - Risk of Corrosion, Low - Risk of Static)
[ ] Storage Compliance Checks Performed (Dust-free environment verified, Moisture/Humidity control active, Temperature stability confirmed, Organized/Labeled shelving)
[ ] Observed Environmental Anomalies
[ ] Environmental Sensor Log/Photo Evidence
[ ] Inspector Verification

--- CLEANING & LUBRICATION MAINTENANCE RECORDS ---
[ ] Last Cleaning Date
[ ] Cleaning Agent Used (Degreaser, Isopropanol, Specialized Solvent, Distilled Water, Other)
[ ] Lubrication Points Addressed (Moving Joints, Threaded Components, Bearing Surfaces, Pneumatic Cylinders)
[ ] Quantity of Tools Serviced
[ ] Maintenance Observations & Discrepancies
[ ] Maintenance Log Photo Evidence
[ ] Technician Verification

--- POST-INSPECTION DOCUMENTATION & REPORTING ---
[ ] Inspection Completion Date
[ ] Overall Inspection Status (Passed, Passed with Minor Non-Compliance, Failed - Immediate Action Required)
[ ] Summary of Non-Compliance Issues
[ ] Upload Calibration Certificate Photos
[ ] Lead Workshop Supervisor Signature

--- END OF TEMPLATE ---
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