SECURITY CAMERA FUNCTIONALITY CHECKLIST

Created by ChecklistGuro (https://checklistguro.com)

--- CAMERA SYSTEM INITIALIZATION & BASIC OPERATION ---
[ ] Camera Firmware Version
[ ] Initial Camera Status (Online/Offline) (Online, Offline)
[ ] Date of Last System Reboot
[ ] Time of Last System Reboot
[ ] Network Connection Status (Connected/Disconnected) (Connected, Disconnected)
[ ] IP Address Configuration (Static/DHCP)
[ ] Number of Cameras Successfully Connected
[ ] Any Initialization Errors Encountered?

--- IMAGE QUALITY & CLARITY ---
[ ] Lux Rating Verification (actual vs. specified)
[ ] Image Color Accuracy (Excellent, Good, Fair, Poor)
[ ] Image Sharpness (Excellent, Good, Fair, Poor)
[ ] Describe any visual artifacts or distortions observed.
[ ] Frame Rate (FPS) verification
[ ] Night Vision Performance (if applicable) (Excellent, Good, Fair, Poor, Not Applicable)
[ ] Lens Distortion Correction (if applicable)

--- PAN-TILT-ZOOM (PTZ) FUNCTIONALITY (IF APPLICABLE) ---
[ ] PTZ Control Method Verification (Manual Control, Automated Patrol, Software Interface, All Methods)
[ ] Pan Range (Degrees)
[ ] Tilt Range (Degrees)
[ ] Zoom Range (Optical)
[ ] PTZ Speed Response (Fast, Normal, Slow, Acceptable, Unacceptable)
[ ] Describe any observed PTZ Movement Issues
[ ] Patrol Route Accuracy (If Applicable) (Accurate, Slight Deviation, Significant Deviation, Not Applicable)
[ ] Last PTZ Calibration Date/Time

--- RECORDING & STORAGE ---
[ ] Maximum Recording Capacity (GB/TB)
[ ] Current Storage Used (GB/TB)
[ ] Remaining Storage Capacity (GB/TB)
[ ] Recording Type (Continuous/Event-Triggered/Scheduled) (Continuous, Event-Triggered, Scheduled)
[ ] Recording Retention Period (Days/Weeks/Months) (Days, Weeks, Months)
[ ] Number of Backup Copies (If Applicable)
[ ] Last Successful Data Backup Date
[ ] Notes/Comments Regarding Recording & Storage Performance

--- NETWORK CONNECTIVITY & REMOTE ACCESS ---
[ ] Network Bandwidth Utilization (Average)
[ ] Connection Type (Wired/Wireless) (Wired, Wireless)
[ ] Remote Access URL/IP Address
[ ] Ping Response Time (ms)
[ ] Authentication Method Used (Username/Password, Two-Factor Authentication, Other)
[ ] Notes on Remote Access Experience (Stability, Lag, etc.)
[ ] Firewall Configuration Verified? (Yes, No, N/A)

--- ALERTS & NOTIFICATIONS ---
[ ] Motion Detection Alert Test (Successful, Partial Success (False Positive), Failed)
[ ] Scheduled Alert Test Time (e.g., for nighttime tests)
[ ] Audio Alert Test (if applicable) (Successful, Partial Success (Low Volume), Failed)
[ ] Notification Delay (seconds)
[ ] Email Notification Test (Successful, Failed, Not Configured)
[ ] Comments/Observations Regarding Alerts

--- POWER & BACKUP SYSTEMS ---
[ ] UPS Battery Capacity (in Amp-Hours)
[ ] UPS Battery Voltage (in Volts)
[ ] UPS Runtime (in minutes) under typical load
[ ] Last UPS Battery Replacement Date
[ ] Generator Status (if applicable) (Operational, Needs Maintenance, Not Applicable)
[ ] Automatic Transfer Switch (ATS) Functionality (if applicable) (Functional, Needs Testing, Not Applicable)
[ ] Notes on Power Backup System Observations

--- SYSTEM INTEGRATION (IF APPLICABLE) ---
[ ] Integrated System Type (Access Control System, Alarm System, Building Management System (BMS), None, Other)
[ ] Description of Integration Points
[ ] Integration Communication Protocol (ONVIF, RS-485, TCP/IP, Proprietary, Other)
[ ] Latency (ms) - Integration Response Time
[ ] Describe any issues encountered during integration testing.
[ ] Event Triggering Validation (Successful, Partial, Failed)

--- SOFTWARE & FIRMWARE ---
[ ] Current Firmware Version
[ ] Firmware Update Status (Up-to-Date, Outdated, Pending Update)
[ ] Last Firmware Update Date
[ ] Notes on Last Firmware Update (if applicable)
[ ] Software Compatibility (NVR/DVR) (Compatible, Incompatible, Needs Verification)
[ ] Software Version of NVR/DVR (if applicable)
[ ] Available Storage Space (GB)

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/retail/security-camera-functionality-checklist
(Click "Install Template" to launch your digital inspection tool immediately)