SMART GRID LOAD BALANCING PROCESS

Created by ChecklistGuro (https://checklistguro.com)

[ ] Fetch Current Grid Load: Retrieve real-time energy consumption data from the Grid_Status data model.
[ ] Fetch Available Supply: Retrieve current energy production levels from Renewable_Sources data model.
[ ] Fetch Demand Forecast: Retrieve predicted energy demand from Forecast_Data data model.
[ ] Calculate Total Demand: Sum all predicted load entries from the Demand_Forecast data model to get total required load.
[ ] Calculate Total Supply: Sum all available energy from the Renewable_Sources data model.
[ ] Calculate Load Imbalance: Subtract Total Supply from Total Demand to determine the deficit or surplus.
[ ] Calculate Threshold Alert: Determine if the Load Imbalance exceeds the predefined safety threshold percentage.
[ ] Assign Grid Operator Review: Create a task for the Grid_Engineer to review the imbalance if the threshold is exceeded.
[ ] Update Grid Status: Update the 'Status' field in the Grid_Status data model to 'Critical' or 'Stable'.
[ ] Log Balancing Event: Create a new entry in the Load_Balancing_Logs data model documenting the imbalance details.
[ ] Execute Load Shedding Protocol: Create a high-priority task for the Automation_System to reduce load from non-essential sectors.
[ ] Adjust Battery Storage: Update the 'Discharge_Rate' field in the Battery_Storage data model to inject power into the grid.
[ ] Notify Stakeholders: Send an email alert to the Utility_Management group regarding the load imbalance event.
[ ] Alert Emergency Services: Send an SMS to the Emergency_Response_Team if the imbalance threatens grid stability.
[ ] Generate Daily Stability Report: Create a summary report of all load balancing actions and grid stability metrics for the last 24 hours.

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/workflow-templates/energy/smart-grid-load-balancing-process
(Click "Install Template" to launch your digital inspection tool immediately)