THEME PARK RIDE MAINTENANCE CHECKLIST TEMPLATE

Created by ChecklistGuro (https://checklistguro.com)

--- DAILY VISUAL INSPECTION ---
[ ] Ride Name/Identifier
[ ] Overall Ride Condition Notes (Appearance, unusual sounds)
[ ] Restraint Condition (Excellent, Good, Fair, Poor - Requires Attention)
[ ] Visual Inspection Temperature (degrees Celsius)
[ ] Potential Issues Observed (select all that apply) (Cracks, Corrosion, Leaks, Loose Parts, Unusual Noises, None)
[ ] Inspector Signature

--- MECHANICAL SYSTEM CHECKS ---
[ ] Gear Mesh Clearance (mm)
[ ] Chain Tension (mm)
[ ] Belt Deflection (mm)
[ ] Chain/Belt Condition (Excellent, Good, Fair, Poor)
[ ] Detailed Notes on Mechanical System Condition
[ ] Photo of Mechanical Components

--- ELECTRICAL SYSTEM CHECKS ---
[ ] Voltage (V)
[ ] Current (A)
[ ] Resistance (Ohms)
[ ] Sensor Status (Operational, Faulty, Needs Calibration)
[ ] Wiring Condition (Good, Frayed, Damaged, Corroded)
[ ] Last Calibration Date
[ ] Time of Last Electrical Test

--- HYDRAULIC/PNEUMATIC SYSTEM CHECKS ---
[ ] Hydraulic Fluid Level (inches)
[ ] Pneumatic System Pressure (PSI)
[ ] Fluid Condition (Appearance) (Clear, Cloudy, Milky, Dark/Contaminated)
[ ] Hose Condition (Good, Minor Wear, Cracks/Leaks, Significant Damage)
[ ] Cylinder Extension Speed (inches/second)
[ ] Any Unusual Noises or Behavior?
[ ] Last Hydraulic Filter Change

--- STRUCTURAL INTEGRITY INSPECTION ---
[ ] Support Beam Corrosion Measurement (mm)
[ ] Description of Any Cracks Observed
[ ] Track Alignment Variance (mm)
[ ] Detailed Assessment of Weld Points
[ ] Overall Structural Condition (Excellent, Good, Fair, Poor)
[ ] Photographic Evidence of Damage

--- SAFETY DEVICE TESTING ---
[ ] Restraint System Functionality (Functional, Needs Adjustment, Malfunctioning - Out of Service)
[ ] Emergency Stop Button Functionality (Functional, Needs Adjustment, Malfunctioning - Out of Service)
[ ] Restraint Force (lbs)
[ ] Last Inspection Date (Safety Sensors)
[ ] Time of Safety Sensor Test
[ ] Safety Sensor Calibration Status (Within Calibration, Out of Calibration - Needs Adjustment)
[ ] Technician Signature (Safety Device Verification)

--- LUBRICATION AND GREASE POINTS ---
[ ] Gearbox Oil Level
[ ] Grease Point 1 - Quantity (grams)
[ ] Grease Point 2 - Quantity (grams)
[ ] Grease Type Used (Lithium Grease, Polyurea Grease, Calcium Sulfonate Grease, Other)
[ ] Notes on Lubrication
[ ] Last Lubrication Date

--- OPERATIONAL TESTING ---
[ ] Start Time of Test Cycle
[ ] Cycle Speed (RPM)
[ ] Load Capacity (lbs/kg)
[ ] Noise Level Assessment (Normal, Slightly Elevated, Elevated - Investigate)
[ ] Vibration Assessment (Normal, Slightly Elevated, Elevated - Investigate)
[ ] Observations During Test Cycle
[ ] End Time of Test Cycle

--- DOCUMENTATION & RECORD KEEPING ---
[ ] Date of Inspection
[ ] Time of Inspection
[ ] Ride Operating Hours Since Last Inspection
[ ] Detailed Notes/Observations
[ ] Overall Ride Condition (Post-Inspection) (Excellent, Good, Fair, Poor, Needs Repair)
[ ] Inspector Signature
[ ] Attach Photo Documentation (if applicable)

--- SCHEDULED PREVENTATIVE MAINTENANCE ---
[ ] Last Gearbox Oil Change
[ ] Motor Operating Hours
[ ] Cycle Counter Reads
[ ] Hydraulic Fluid Level (Normal, Low, High)
[ ] Supporting Documentation/Photos
[ ] Next Brake Pad Replacement (if applicable)
[ ] Notes/Observations

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/maintenance-management/theme-park-ride-maintenance-checklist-template
(Click "Install Template" to launch your digital inspection tool immediately)