TOOLING MANAGEMENT WORKFLOW FOR MANUFACTURING

Created by ChecklistGuro (https://checklistguro.com)

[ ] Get Existing Tooling Records: Retrieve all current tooling records from the Tooling Management Data Model.
[ ] Get Upcoming Calibration Dates: Retrieve tooling records with calibration dates within the next 12 months.
[ ] Assign Calibration Task: Create a task for the assigned technician to perform the calibration.
[ ] Calibration Reminder Email: Send an email reminder to the technician and tooling owner prior to calibration date.
[ ] Update Calibration Status: Update the 'Calibration Status' field in the Tooling Management Data Model after completion.
[ ] Assign Inspection Task: Create a task to inspect the tooling for wear or damage after calibration.
[ ] Create New Tooling Record: Create a new entry in the Tooling Management Data Model when new tooling is introduced.
[ ] Update Tooling Location: Update the Tooling Management Data Model with the current location of the tooling.
[ ] Calculate Remaining Calibration Time: Calculate the remaining time until the next scheduled calibration, based on the 'Last Calibration Date' and 'Calibration Frequency'.
[ ] Generate Tooling Inventory Report: Create a report of all tooling records, including status, location, and upcoming calibration dates.
[ ] Get Tooling Requiring Repair: Retrieve tooling records flagged for repair or maintenance.
[ ] Assign Repair Task: Create a task to have a repair made to the tool.
[ ] Update Tooling Repair Status: Update the tooling repair status in the tooling data model.
[ ] Archive Retired Tooling: Archive tooling records that are no longer in use (maintaining historical data).

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/workflow-templates/manufacturing/tooling-management-workflow-for-manufacturing
(Click "Install Template" to launch your digital inspection tool immediately)