TRAIN LEVEL CROSSING SAFETY INSPECTION CHECKLIST TEMPLATE

Created by ChecklistGuro (https://checklistguro.com)

--- GENERAL INFORMATION ---
[ ] Inspection Date
[ ] Inspection Time
[ ] Crossing Location (GPS Coordinates)
[ ] Crossing Type (Public Road, Private Road, Rail Trail)
[ ] Crossing Identifier (e.g., milepost)
[ ] Inspector Name
[ ] Agency/Company

--- CROSSING SIGNALS AND LIGHTS ---
[ ] Last Signal Test Time
[ ] Signal Head Brightness (Lumens)
[ ] Flashing Rate (Flashes Per Minute)
[ ] Signal Alignment (Correct, Slightly Misaligned, Significantly Misaligned)
[ ] Light Functionality (All Lights Functioning, Red Light Malfunctioning, Yellow Light Malfunctioning, Green Light Malfunctioning)
[ ] Last Bulb Replacement Date
[ ] Notes on Signal Performance

--- GATES AND BARRIERS ---
[ ] Gate Opening Speed (seconds)
[ ] Barrier Closing Speed (seconds)
[ ] Gate/Barrier Material (Steel, Aluminum, Wood, Composite)
[ ] Gate/Barrier Operation Mode (Automatic, Manual, Semi-Automatic)
[ ] Description of any unusual noises during operation
[ ] Condition of Barrier Chain/Link (if applicable) (Excellent, Good, Fair, Poor)
[ ] Date of last gate/barrier maintenance

--- WARNING SIGNS AND MARKINGS ---
[ ] Sign Condition (Overall) (Excellent, Good, Fair, Poor)
[ ] Sign Reflectivity (Excellent, Good, Fair, Poor)
[ ] Sign Type (e.g., Advance Warning, Crossbucks)
[ ] Sign Size (Width in inches)
[ ] Sign Size (Height in inches)
[ ] Sign Legibility (Distance) (< 100ft, 100-200ft, 200-300ft, > 300ft)
[ ] Notes on Sign Damage (Rust, Fading, etc.)

--- TRACK GEOMETRY AND ALIGNMENT ---
[ ] Track Superlevation (mm)
[ ] Track Alignment Variance (mm)
[ ] Curve Radius (meters)
[ ] Track Condition (Good, Fair, Poor)
[ ] Detailed Observations (e.g., visible cracks, dips)
[ ] Exact Location of Geometry Deviation

--- APPROACH ROAD VISIBILITY ---
[ ] Distance to Crossing Visible (meters)
[ ] Road Grade (%)
[ ] Road Surface Condition (Dry, Wet, Snow/Ice, Oil/Gravel)
[ ] Presence of Obstructions (e.g., trees, signs) (None, Minor, Significant)
[ ] Detailed Observations regarding Visibility
[ ] GPS Coordinates of Obstruction (if applicable)

--- VEGETATION CLEARANCE ---
[ ] Distance to Trackside Vegetation (meters)
[ ] Vegetation Types Observed (Trees, Shrubs, Grass, Weeds, Other)
[ ] Description of Vegetation Conditions
[ ] Height of Vegetation at Obstruction Point (meters)
[ ] Visibility of Crossing Lights/Signs (Clear, Partially Obstructed, Completely Obstructed)
[ ] Photo Evidence of Vegetation

--- EMERGENCY EQUIPMENT ---
[ ] Emergency Call Volume (Last 24 Hours)
[ ] Communication System Status (Operational, Degraded, Out of Service)
[ ] Last Battery Replacement (Emergency Phone)
[ ] Last System Test Time
[ ] Backup Power Status (Operational, Degraded, Out of Service)
[ ] Notes on Emergency Equipment Condition

--- MAINTENANCE RECORDS ---
[ ] Last Signal Maintenance Date
[ ] Last Gate/Barrier Maintenance Date
[ ] Gate Cycle Count (Since Last Maintenance)
[ ] Maintenance Performed (Select All That Apply) (Signal Repair, Gate/Barrier Repair, Sign Replacement, Track Alignment, Vegetation Control, Other)
[ ] Detailed Description of Maintenance Activities
[ ] Attach Maintenance Reports/Photos
[ ] Signal Voltage (During Test)

--- DEFICIENCIES AND RECOMMENDATIONS ---
[ ] Detailed Description of Deficiency
[ ] Severity Rating (1-10)
[ ] Immediate Action Required? (Yes, No)
[ ] Target Completion Date
[ ] Estimated Repair Cost
[ ] Assigned Responsibility (Maintenance Team, Engineering Department, External Contractor)
[ ] Additional Notes/Comments
[ ] Inspector Signature

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/public-transport-management/train-level-crossing-safety-inspection-checklist-template
(Click "Install Template" to launch your digital inspection tool immediately)