TRAIN ROLLING STOCK CONDITION REPORT CHECKLIST TEMPLATE

Created by ChecklistGuro (https://checklistguro.com)

--- EXTERIOR BODYWORK ---
[ ] Overall Body Condition Score (1-10)
[ ] Presence of Dents? (Yes, No)
[ ] Presence of Scratches? (Yes, No)
[ ] Condition of Paintwork (Excellent, Good, Fair, Poor)
[ ] Detailed Description of any Damage
[ ] Number of Visible Graffiti Instances
[ ] Upload Photos of Bodywork

--- INTERIOR CONDITION ---
[ ] Seat Cleanliness Score (1-5)
[ ] Flooring Condition (Excellent, Good, Fair, Poor)
[ ] Notes on Graffiti or Vandalism
[ ] HVAC Functionality (Working Properly, Cooling Issue, Heating Issue, Not Working)
[ ] Number of Damaged Seats
[ ] Damaged Interior Components (Select all that apply) (Window, Seat, Wall Panel, Floor, Ceiling, Handrail)
[ ] Detailed description of any odors or unpleasant smells

--- MECHANICAL SYSTEMS ---
[ ] Engine Hours
[ ] Transmission Fluid Level (inches)
[ ] Brake Pad Thickness (Left) (Within Spec, Low, Needs Replacement)
[ ] Brake Pad Thickness (Right) (Within Spec, Low, Needs Replacement)
[ ] Suspension Spring Condition Rating (1-5, 5=Excellent)
[ ] Notes on Engine Performance
[ ] Coolant Level (Full, Low, Empty)
[ ] Attach Photo of Undercarriage

--- ELECTRICAL SYSTEMS ---
[ ] Battery Voltage (V)
[ ] HVAC System Power Consumption (kW)
[ ] Lighting Functionality (Fully Functional, Minor Issues, Major Issues)
[ ] Communication System Checks (PA System, Wi-Fi, GPS, Passenger Information Displays)
[ ] Emergency Lighting Status (Functional, Needs Inspection)
[ ] Last Electrical System Overhaul Date

--- UNDERFRAME & BOGIES ---
[ ] Bogie Serial Number 1
[ ] Bogie Serial Number 2
[ ] Axle Bearing Temperature (Left)
[ ] Axle Bearing Temperature (Right)
[ ] Suspension Condition (Good, Fair, Poor)
[ ] Gearbox Oil Level (Full, Low, Empty)
[ ] Any unusual noises or vibrations observed?
[ ] Attach any relevant photos (e.g., corrosion)

--- DOORS & WINDOWS ---
[ ] Number of Doors Functioning Correctly
[ ] Number of Windows Intact
[ ] Door Operation (Left Door) (Fully Functional, Minor Issue, Malfunctioning, Unable to Operate)
[ ] Door Operation (Right Door) (Fully Functional, Minor Issue, Malfunctioning, Unable to Operate)
[ ] Window Condition (General) (Clear, Minor Scratch, Crack, Shattered)
[ ] Detailed Description of any Door/Window Issues
[ ] Last Maintenance Date (Doors)

--- SAFETY EQUIPMENT ---
[ ] Fire Extinguisher Quantity
[ ] Last Fire Extinguisher Inspection Date
[ ] Emergency Hammer Condition (Intact, Damaged, Missing)
[ ] Operational Emergency Exits (Exit 1, Exit 2, Exit 3, Exit 4)
[ ] Passenger Information System Functionality (Functional, Malfunctioning, Not Present)
[ ] Comments on Safety Equipment

--- WHEEL & BRAKE CONDITION ---
[ ] Wheel Profile Deviation (mm)
[ ] Brake Pad Thickness (mm) - Left
[ ] Brake Pad Thickness (mm) - Right
[ ] Brake Disc/Drum Condition (Good, Fair, Poor, Requires Replacement)
[ ] Wheel Condition (Good, Fair, Poor, Requires Re-profiling)
[ ] Detailed Notes on Wheel/Brake Condition
[ ] Date of Last Brake Service
[ ] Wheel Diameter (mm)

--- AIR CONDITIONING/HEATING SYSTEM ---
[ ] Supply Air Temperature (Cooling) - °C
[ ] Return Air Temperature (Cooling) - °C
[ ] Supply Air Temperature (Heating) - °C
[ ] Return Air Temperature (Heating) - °C
[ ] Cooling System Operation (Normal, Degraded, Faulted)
[ ] Heating System Operation (Normal, Degraded, Faulted)
[ ] Observed Issues / Notes
[ ] Last Maintenance Date

--- OVERALL OPERATIONAL READINESS ---
[ ] Overall Serviceability Rating (Excellent, Good, Fair, Poor, Unserviceable)
[ ] Estimated Time Until Next Scheduled Maintenance
[ ] Summary of Findings & Recommendations
[ ] Date of Next Inspection
[ ] Potential for Immediate Return to Service? (Yes, No, Conditional - Requires Minor Repairs)
[ ] Inspector Signature

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/public-transport-management/train-rolling-stock-condition-report-checklist-template
(Click "Install Template" to launch your digital inspection tool immediately)