TRAIN STATION SECURITY INSPECTION CHECKLIST TEMPLATE

Created by ChecklistGuro (https://checklistguro.com)

--- PERIMETER SECURITY ---
[ ] Fence Height (meters)
[ ] Gate Condition (Excellent, Good, Fair, Poor)
[ ] Gate Locking Mechanism (Functional, Malfunctioning)
[ ] Description of any perimeter breaches or damage
[ ] Date of last perimeter maintenance

--- CCTV SURVEILLANCE ---
[ ] Camera ID
[ ] Camera Functionality (Operational, Malfunctioning, Needs Repair)
[ ] Frame Rate (FPS)
[ ] Recording Status (Recording, Not Recording, Needs Verification)
[ ] Last Maintenance Date
[ ] Any Unusual Activity Noted

--- LIGHTING ---
[ ] Ambient Light Level (Lux) - Platform 1
[ ] Ambient Light Level (Lux) - Concourse
[ ] Ambient Light Level (Lux) - Stairwells
[ ] Light Fixture Condition - Platform 1 (Excellent, Good, Fair, Poor)
[ ] Emergency Lighting Functionality - Main Entrance (Functional, Not Functional, Needs Testing)
[ ] Last Lighting Maintenance Date
[ ] Notes on Lighting Issues

--- ACCESS CONTROL ---
[ ] Gate/Turnstile Functionality (Fully Operational, Partially Operational, Non-Operational)
[ ] Number of Access Points Secured
[ ] Keypad/Card Reader Status (Functional, Malfunctioning, Needs Repair)
[ ] Last Access Control System Maintenance
[ ] Access Control User Verification Methods (Biometrics, Keycards, PIN Codes, Manual Authorization)
[ ] Authorized Personnel List Checked?
[ ] Location of Access Control Panel

--- EMERGENCY EXITS ---
[ ] Exit Light Condition (0-10, 10 being best)
[ ] Exit Sign Visibility (Excellent, Good, Fair, Poor)
[ ] Emergency Door Functionality (Opens Freely, Requires Force, Malfunctioning)
[ ] Last Exit Route Drills Conducted
[ ] Time of last check of emergency lights
[ ] Comments on Exit Conditions
[ ] Obstructions in Exit Pathway (None, Minor, Significant)

--- FIRE SAFETY EQUIPMENT ---
[ ] Fire Extinguisher A Count
[ ] Fire Extinguisher B Count
[ ] Fire Extinguisher C Count
[ ] Fire Extinguisher Inspection Date (Last) (Within last month, Within last 3 months, More than 3 months ago)
[ ] Next Fire Extinguisher Inspection Date
[ ] Fire Alarm System Status (Operational, Needs Repair, Under Maintenance)
[ ] Sprinkler System Pressure (PSI)
[ ] Comments/Observations (Fire Safety)

--- HAZARDOUS MATERIALS ---
[ ] Description of Hazardous Materials Present
[ ] Quantity of Chemicals (e.g., liters, kilograms)
[ ] Storage Condition (e.g., temperature controlled, ventilated) (Temperature Controlled, Ventilated, Uncontrolled)
[ ] Hazards Identified (e.g., flammable, corrosive, toxic) (Flammable, Corrosive, Toxic, Reactive, Oxidizing)
[ ] Date of Last Inspection
[ ] Exact Location of Hazardous Materials

--- SECURITY PERSONNEL ---
[ ] Number of Security Personnel Present
[ ] Uniform Compliance (Compliant, Minor Deviation, Significant Deviation)
[ ] Communication Equipment Functionality (Functional, Minor Issue, Non-Functional)
[ ] Observations Regarding Patrol Frequency and Effectiveness
[ ] Response to Simulated Incident (if applicable) (Appropriate & Timely, Delayed Response, Inadequate Response)
[ ] Last Patrol Log Review Date

--- PUBLIC ANNOUNCEMENTS ---
[ ] Emergency Announcement System Functionality (Functional, Partially Functional, Not Functional)
[ ] Last System Test Time
[ ] Content of Standard Emergency Announcements
[ ] Clarity of Announcements (Excellent, Good, Fair, Poor)
[ ] Date of Last Content Review
[ ] Volume Level (dB)
[ ] Public Address System Backup (Available and Tested, Available but not Tested, Not Available)

--- REPORTING & DOCUMENTATION ---
[ ] Inspection Date
[ ] Inspection Time Started
[ ] Inspection Time Ended
[ ] Temperature (for environmental records)
[ ] Summary of Findings
[ ] Supporting Documentation (Photos, Reports)
[ ] Overall Risk Level (Low, Medium, High)
[ ] Inspector Name
[ ] Inspector Signature

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/public-transport-management/train-station-security-inspection-checklist-template
(Click "Install Template" to launch your digital inspection tool immediately)