TRAM MAINTENANCE & INSPECTION CHECKLIST TEMPLATE - PUBLIC TRANSIT

Created by ChecklistGuro (https://checklistguro.com)

--- PRE-OPERATION INSPECTION ---
[ ] Date of Inspection
[ ] Time of Inspection
[ ] Tram Number/Fleet ID
[ ] Shift/Route Assigned (Morning Shift, Afternoon Shift, Night Shift)
[ ] Overall Pre-Operation Condition (Excellent, Good, Fair, Poor)
[ ] Additional Notes/Comments (Pre-Operation)
[ ] Inspector Signature

--- BRAKE SYSTEM INSPECTION ---
[ ] Brake Cylinder Pressure (PSI)
[ ] Brake Pipe Pressure (PSI)
[ ] Brake Pad Thickness (mm) (< 3mm - Replacement Required, 3-6mm - Monitoring Required, > 6mm - Acceptable)
[ ] Brake Shoe Condition (Good, Fair - Minor Wear, Poor - Significant Wear)
[ ] Notes on Brake Performance
[ ] ABS Functionality Test Result (Passed, Failed, Not Tested)
[ ] Emergency Brake Application Distance (meters)
[ ] Leakage Inspection Result

--- WHEEL AND RAIL INTERACTION ---
[ ] Wheel Profile Wear (mm)
[ ] Rail Gauge (mm)
[ ] Wheel Condition (Good, Fair, Poor)
[ ] Rail Condition (Good, Fair, Poor)
[ ] Notes on Wheel/Rail Interaction
[ ] Wheel Flatness (mm)

--- TRACTION SYSTEM ---
[ ] Motor Temperature (Celsius)
[ ] Gearbox Oil Level (mm)
[ ] Gearbox Oil Condition (Good, Fair, Poor, Needs Replacement)
[ ] Motor Current Draw (Amps)
[ ] Traction Motor Noise (Normal, Slightly Elevated, Excessive, Unusual)
[ ] Notes on Traction System Performance
[ ] Last Traction Motor Serviced

--- ELECTRICAL SYSTEMS ---
[ ] Battery Voltage (V)
[ ] Charging Current (A)
[ ] Lighting System Condition (Working Properly, Dim/Flickering, Not Working)
[ ] Wiring Issues Found? (Exposed Wires, Damaged Insulation, Loose Connections, None)
[ ] Detailed Description of Electrical Issues (if any)
[ ] Last Battery Service Date

--- AIR CONDITIONING & VENTILATION ---
[ ] Supply Air Temperature (C)
[ ] Return Air Temperature (C)
[ ] Airflow Rate (mÂ³/h)
[ ] Air Filter Condition (Excellent, Good, Fair, Poor)
[ ] Refrigerant Pressure (Nominal, High, Low)
[ ] Notes/Observations

--- PASSENGER INFORMATION SYSTEM (PIS) ---
[ ] Next Station Display Accuracy (seconds)
[ ] Audio Announcements Functionality (Working Correctly, Partially Working, Not Working)
[ ] Visual Destination Display Functionality (Working Correctly, Partially Working, Not Working)
[ ] Description of any PIS Malfunctions
[ ] Last PIS Software Update Date
[ ] Emergency Messaging Display Functionality (Working Correctly, Partially Working, Not Working)

--- DOOR OPERATION ---
[ ] Door Opening/Closing Time (seconds)
[ ] Door Operation Mode (Automatic, Manual, Timed)
[ ] Door Sensor Functionality (Functional, Needs Repair, Not Present)
[ ] Comments on Door Operation (e.g., unusual noises, jerky movement)
[ ] Number of Door Open/Close Cycles Observed
[ ] Accessibility Features Working (e.g., ramp/lift) (Yes, No, N/A)
[ ] Inspector Signature

--- BODYWORK AND INTERIOR ---
[ ] Windscreen Chip Depth (mm)
[ ] Interior Cleanliness (Rating) (Excellent, Good, Fair, Poor)
[ ] Description of Bodywork Damage (if any)
[ ] Seat Condition (General) (Excellent, Good, Fair, Poor)
[ ] Number of Vandalism Incidents Noted
[ ] Details of Any Unpleasant Odors Detected

--- SAFETY EQUIPMENT ---
[ ] Fire Extinguisher Pressure (PSI)
[ ] Fire Extinguisher Inspection Status (Pass, Fail, N/A)
[ ] Emergency Hammer Condition (Good, Damaged, Missing)
[ ] First Aid Kit Completeness (Complete, Incomplete, N/A)
[ ] Last Fire Drill Date
[ ] Inspector Signature

--- MISCELLANEOUS ---
[ ] Additional Notes/Observations
[ ] Mileage at Inspection
[ ] Next Scheduled Maintenance Date
[ ] Overall Condition Assessment (Excellent, Good, Fair, Poor)
[ ] Attach Photos/Documents (Optional)
[ ] Inspection Location

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/public-transport-management/tram-maintenance-inspection-checklist-template-public-transit
(Click "Install Template" to launch your digital inspection tool immediately)