TRAM TRACK INSPECTION & MAINTENANCE CHECKLIST TEMPLATE

Created by ChecklistGuro (https://checklistguro.com)

--- VISUAL TRACK CONDITION ---
[ ] Overall Track Condition Rating (1-5, 5=Excellent)
[ ] Description of General Appearance
[ ] Presence of Surface Rust (Yes, No, Minor, Moderate)
[ ] Presence of Vegetation Overgrowth (Yes, No)
[ ] Photos of Track Condition
[ ] Estimated Track Length Inspected (meters)
[ ] Date of Inspection

--- RAIL HEAD & PROFILE ---
[ ] Maximum Rail Head Wear (mm)
[ ] Average Rail Head Depth (mm)
[ ] Rail Profile Type (Standard Profile, Wear Resistant Profile, Other)
[ ] Description of any rail profile irregularities
[ ] Grinding Depth (if applicable, mm)
[ ] Presence of Head Checks (Yes, No, Unsure)
[ ] Rib Height (mm)

--- FASTENERS & BASEPLATES ---
[ ] Fastener Torque (Nm)
[ ] Baseplate Condition (Good, Fair, Poor)
[ ] Number of Corroded Fasteners
[ ] Fastener Type (Type A, Type B, Type C)
[ ] Detailed Notes on Baseplate Integrity
[ ] Number of Loose Fasteners

--- SLEEPERS / TIES ---
[ ] Sleeper Spacing (mm)
[ ] Sleeper Material (Concrete, Wood, Composite)
[ ] Sleeper Condition (Excellent, Good, Fair, Poor)
[ ] Number of Cracked/Damaged Sleepers
[ ] Description of any sleeper damage or defects
[ ] Date of Last Sleeper Replacement/Repair
[ ] Sleeper Fixation Type (Baseplate, Direct Fix, Other)

--- BALLAST ---
[ ] Ballast Depth (cm)
[ ] Ballast Cleanliness Score (1-5, 1=Very Dirty, 5=Very Clean)
[ ] Ballast Type (Crushed Stone, Chat, Other)
[ ] Observations regarding ballast condition (e.g., compaction, fouling)
[ ] Types of Contaminants Present (Vegetation, Debris, Soil, Other)
[ ] Ballast Compaction Percentage (%)
[ ] Drainage Assessment (Good, Fair, Poor)

--- GEOMETRIC ALIGNMENT ---
[ ] Track Gauge (mm)
[ ] Curve Radius (m)
[ ] Superlevation (mm)
[ ] Longitudinal Slope (%)
[ ] Alignment Condition (Within Tolerance, Minor Deviation, Significant Deviation)
[ ] Date of Last Survey
[ ] Survey Location (GPS Coordinates)

--- SWITCH & CROSSING INSPECTION ---
[ ] Switch Point Gap (mm)
[ ] Frog Wear (mm)
[ ] Switch Mechanism Operation (Smooth, Jerky, Sticking, Not Operational)
[ ] Switch Lock Status (Locked, Unlocked, Damaged)
[ ] Any Unusual Noises During Operation?
[ ] Last Switch Replacement Date
[ ] Potential Issues Observed (Corrosion, Wear, Loose Fasteners, Misalignment, None)
[ ] GPS Location of Switch

--- DRAINAGE SYSTEMS ---
[ ] Outlet Flow Rate (L/s)
[ ] Outlet Condition (Clear, Partially Blocked, Completely Blocked)
[ ] Description of any Blockage (if applicable)
[ ] Culvert Condition (Good, Fair, Poor)
[ ] Last Cleaning Date
[ ] GPS Location of Culvert Outlet

--- VEGETATION CONTROL ---
[ ] Vegetation Height (cm)
[ ] Vegetation Types Present (Grass, Weeds, Shrubs, Trees, Other)
[ ] Detailed Description of Vegetation Issues
[ ] Location of Significant Vegetation Overgrowth
[ ] Date of Last Vegetation Clearance
[ ] Vegetation Control Method Used (Manual Trimming, Herbicide Application, Mechanical Cutting, Other)

--- RECORD KEEPING & DOCUMENTATION ---
[ ] Date of Inspection
[ ] Time of Inspection
[ ] Inspection Route Mileage / Location Code
[ ] Summary of Findings & Observations
[ ] Supporting Photos/Videos
[ ] Inspection Status (Pass, Fail, Conditional Pass)
[ ] Inspector Name
[ ] Inspector Signature

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/public-transport-management/tram-track-inspection-maintenance-checklist-template
(Click "Install Template" to launch your digital inspection tool immediately)