TRAM WHEEL & RAIL INSPECTION CHECKLIST TEMPLATE

Created by ChecklistGuro (https://checklistguro.com)

--- GENERAL INFORMATION ---
[ ] Inspection Date
[ ] Inspection Time
[ ] Inspection Location (Tram Route/Section)
[ ] Inspector Role (Track Inspector, Wheelset Inspector, Maintenance Supervisor)
[ ] Inspector Name
[ ] Tram Car Number

--- WHEEL CONDITION ---
[ ] Wheel Diameter (mm)
[ ] Tread Depth (mm)
[ ] Flange Condition (Excellent, Good, Fair, Poor)
[ ] Surface Condition Notes
[ ] Wheel Profile (Nominal, Undercut, Overcut)
[ ] Wheel Surface Image

--- RAIL CONDITION ---
[ ] Rail Profile Depth (mm)
[ ] Rail Head Wear (mm)
[ ] Rail Corrosion Level (None, Minor, Moderate, Severe)
[ ] Rail Cracking Presence (No, Yes)
[ ] Description of Rail Defects
[ ] Rail CWR Tension (kN)
[ ] Rail Flange Condition (Good, Fair, Poor)

--- GAUGE MEASUREMENT ---
[ ] Gauge Measurement 1 (mm)
[ ] Gauge Measurement 2 (mm)
[ ] Gauge Measurement 3 (mm)
[ ] Average Gauge (mm)
[ ] Gauge Within Tolerance? (Yes, No)
[ ] Tolerance Limits (mm)
[ ] Comments on Gauge Measurement

--- ALIGNMENT & WEAR PATTERNS ---
[ ] Lateral Movement (mm)
[ ] Vertical Movement (mm)
[ ] Wear Pattern - Wheel Tread (Uniform, Patchy, Cupping, Other)
[ ] Wear Pattern - Rail Head (Uniform, Ribboning, Kestraling, Other)
[ ] Detailed Description of Observed Patterns
[ ] Specific Location of Misalignment (e.g., Curve #)
[ ] Photo of Wheel/Rail Profile

--- CONTAMINATION & DEBRIS ---
[ ] Type of Contamination Present (Dirt/Mud, Oil/Grease, Stone/Gravel, Vegetation, None)
[ ] Estimated Quantity of Debris (Scale of 1-10)
[ ] Detailed Description of Debris/Contamination
[ ] Photo Evidence of Contamination
[ ] Source of Contamination (if known) (Roadway, Environment, Unknown)

--- LUBRICATION ---
[ ] Grease Temperature (Â°C)
[ ] Grease Application Rate (grams/wheel)
[ ] Grease Type (Lithium Grease, Calcium Sulfonate Grease, Other (Specify))
[ ] Notes on Grease Condition (Color, Consistency)
[ ] Last Lubrication Date
[ ] Lubrication Method (Manual, Automated, Other)

--- CORRECTIVE ACTIONS ---
[ ] Detailed Description of Corrective Action Required
[ ] Estimated Cost of Corrective Action (in local currency)
[ ] Priority Level (High, Medium, Low) (High, Medium, Low)
[ ] Target Completion Date
[ ] Assigned Department (Maintenance, Track, etc.) (Maintenance, Track, Signals, Other)
[ ] Estimated Time to Complete (in hours)
[ ] Notes or Comments Regarding Corrective Action

--- PHOTOGRAPHIC EVIDENCE ---
[ ] Overall Wheel Condition - Photo 1
[ ] Wheel Tread Detail - Photo 2
[ ] Wheel Flange Detail - Photo 3
[ ] Rail Surface Condition - Photo 3
[ ] Rail Wear Pattern (if applicable) - Photo 4
[ ] Photo Location (GPS Coordinates)

--- END OF TEMPLATE ---
Transform this text into a digital, automated, and trackable mobile app!
Visit: https://checklistguro.com/templates/public-transport-management/tram-wheel-rail-inspection-checklist-template
(Click "Install Template" to launch your digital inspection tool immediately)